{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["危险性较大分部分项工程汇总表"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":2,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"危险性较大分部分项工程汇总表","index":0,"n_rows":32,"n_cols":21,"rows_kept":32,"cut":false,"hidden":false,"merged":[[0,1,0,22],[1,1,1,22],[2,1,2,13],[2,14,2,18],[2,20,2,22],[3,1,3,2],[3,3,3,22],[4,1,4,2],[4,3,4,11],[4,12,4,13],[4,14,4,22],[5,1,5,22],[6,2,6,4],[6,5,6,19],[6,20,6,22],[7,2,7,4],[7,5,7,19],[7,20,7,22],[8,2,8,4],[8,5,8,19],[8,20,8,22],[9,5,9,19],[9,20,9,22],[10,5,10,19],[10,20,10,22],[11,5,11,19],[11,20,11,22],[12,5,12,19],[12,20,12,22],[13,5,13,19],[13,20,13,22],[14,5,14,19],[14,20,14,22],[15,5,15,19],[15,20,15,22],[16,5,16,19],[16,20,16,22],[17,5,17,19],[17,20,17,22],[18,5,18,19],[18,20,18,22],[19,5,19,19],[19,20,19,22],[20,5,20,19],[20,20,20,22],[21,5,21,19],[21,20,21,22],[22,5,22,19],[22,20,22,22],[23,5,23,19],[23,20,23,22],[24,5,24,19],[24,20,24,22],[25,5,25,19],[25,20,25,22],[26,5,26,19],[26,20,26,22],[27,5,27,19],[27,20,27,22],[28,1,28,5],[28,6,28,10],[28,11,28,15],[28,16,28,22],[29,1,29,4],[29,5,29,10],[29,11,29,15],[29,16,29,22],[30,1,30,10],[30,16,30,22],[31,1,31,22],[0,0,31,0],[9,1,10,1],[11,1,13,1],[14,1,19,1],[20,1,21,1],[22,1,27,1],[9,2,10,4],[11,2,13,4],[14,2,19,4],[20,2,21,4],[22,2,27,4]],"flags":["formulas_cached_only"]}
[null,"危险性较大分部分项工程汇总表"]
[null,"(编制安全专项施工方案)"]
[{"$nulls":14},"GDAQ20111"]
[null," 工程名称:"]
[null," 施工单位:",{"$nulls":10},"监理单位:"]
[]
[null,"序号","分部分项",null,null,"工  程  范  围",{"$nulls":14},"是否含有"]
[null,1,"基坑支护与\r\n降水工程",null,null,"     开挖深度超过3m(含3m)或虽未超过3m,但地质条件和周围环境复杂的基坑\r\n (槽)支护、降水工程"]
[null,2,"土方开挖工程",null,null,"     开挖深度超过3m（含3m）的基坑(槽)的土方开挖工程"]
[null,3,"模板工程及\r\n支撑体系",null,null,"     各类工具式模板工程：包括大模板、滑模、爬模、飞模等工程"]
[{"$nulls":5},"     混凝土模板支撑工程:搭设高度5m及以上；搭设跨度10m及以上；施工总\r\n 荷载10kN/㎡及以上；集中线荷载15kN/m及以上，高度大于支撑水平投影宽度\r\n 且相对独立无联系构件的混凝土模板支撑工程"]
[null,4,"起重吊装及\r\n安装拆卸工程",null,null,"     采用非常规起重设备、方法,且单件起吊重量在10kN及以上的起重吊装工程"]
[{"$nulls":5},"     采用起重机机械进行安装的工程"]
[{"$nulls":5},"     起重机械设备自身的安装、拆卸"]
[null,5,"脚手架工程",null,null,"     搭设高度24m及以上的落地式钢管脚手架工程"]
[{"$nulls":5},"     附着式整体和分片提升脚手架工程"]
[{"$nulls":5},"     悬挑式脚手架工程"]
[{"$nulls":5},"     吊篮脚手架工程"]
[{"$nulls":5},"     自制卸料平台、移动操作平台工程"]
[{"$nulls":5},"     新型及异型脚手架工程"]
[null,6,"拆除、爆破工程",null,null,"     建筑物、构筑物拆除工程"]
[{"$nulls":5},"     采用爆破拆除的工程"]
[null,7,"其他危险性\r\n较大的工程",null,null,"     建筑幕墙安装工程"]
[{"$nulls":5},"     钢结构、网架和索膜结构安装工程"]
[{"$nulls":5},"     人工挖孔桩工程"]
[{"$nulls":5},"     地下暗挖、顶管及水下作业工程"]
[{"$nulls":5},"     预应力工程"]
[{"$nulls":5},"     采用新技术、新工艺、新材料、新设备及尚无相关技术标准的危险性较\r\n 大的分部分项工程"]
[null," 施工总承包单位(公章):",{"$nulls":9},"监理单位项目部(盖章):"]
[null," 项目负责人(签名):",{"$nulls":9},"总监理工程师(签名):"]
[{"$nulls":16},"  年  月  日"]
[null," 注：含有的打“√”，没有的打“×”，由总包单位填写，监理单位确认。"]