{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["超过一定规模的危险性较大分部分项工程汇总表"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":2,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"超过一定规模的危险性较大分部分项工程汇总表","index":0,"n_rows":31,"n_cols":22,"rows_kept":31,"cut":false,"hidden":false,"merged":[[0,1,0,23],[1,1,1,23],[2,1,2,23],[3,1,3,13],[3,14,3,19],[3,21,3,23],[4,1,4,3],[4,4,4,23],[5,1,5,3],[5,4,5,11],[5,12,5,14],[5,15,5,23],[6,1,6,23],[7,2,7,5],[7,6,7,20],[7,21,7,23],[8,6,8,20],[8,21,8,23],[9,6,9,20],[9,21,9,23],[10,6,10,20],[10,21,10,23],[11,6,11,20],[11,21,11,23],[12,6,12,20],[12,21,12,23],[13,6,13,20],[13,21,13,23],[14,6,14,20],[14,21,14,23],[15,6,15,20],[15,21,15,23],[16,6,16,20],[16,21,16,23],[17,6,17,20],[17,21,17,23],[18,6,18,20],[18,21,18,23],[19,6,19,20],[19,21,19,23],[20,6,20,20],[20,21,20,23],[21,6,21,20],[21,21,21,23],[22,6,22,20],[22,21,22,23],[23,6,23,20],[23,21,23,23],[24,6,24,20],[24,21,24,23],[25,6,25,20],[25,21,25,23],[26,6,26,20],[26,21,26,23],[27,1,27,5],[27,6,27,11],[27,12,27,18],[27,19,27,23],[28,1,28,5],[28,6,28,11],[28,12,28,18],[28,19,28,23],[29,1,29,18],[29,19,29,23],[30,1,30,23],[0,0,30,0],[8,1,9,1],[10,1,12,1],[13,1,14,1],[15,1,17,1],[18,1,21,1],[22,1,26,1],[8,2,9,5],[10,2,12,5],[13,2,14,5],[15,2,17,5],[18,2,21,5],[22,2,26,5]],"flags":["formulas_cached_only"]}
[]
[null,"超过一定规模的危险性较大分部分项工程汇总表"]
[null,"(编制安全专项施工方案并组织专家论证)"]
[{"$nulls":14},"GDAQ20112"]
[null," 工程名称:"]
[null," 施工单位:",{"$nulls":10},"监理单位:"]
[]
[null,"序号","分部分项",null,null,null,"工  程  范  围",{"$nulls":14},"是否含有"]
[null,1," 深基坑工程",null,null,null,"     开挖深度超过5m(含5m)的基坑(槽)的土方开挖、支护、降水工程"]
[{"$nulls":6},"     开挖深度不超过5m,但地质条件、周围环境和地下管线复杂,或影响毗\r\n 邻建筑(构筑)物安全的基坑(槽)的土方开挖、支护、降水工程"]
[null,2," 模板工程及支撑\r\n 体系",null,null,null,"     工具式模板工程:包括滑模、爬模、飞模工程\r\n"]
[{"$nulls":6},"     混凝土模板支撑工程:搭设高度8m及以上；搭设跨度18m及以上；施工\r\n 总荷载15kN/㎡及以上；集中线荷载20kN/m及以上"]
[{"$nulls":6},"     承重支撑体系:用于钢结构安装等满堂支撑体系,承受单点集中荷载\r\n 700kg以上"]
[null,3," 起重吊装及安装\r\n 拆卸工程",null,null,null,"     采用非常规起重设备、方法，且单件起吊重量在100kN及以上的起重\r\n 吊装工程"]
[{"$nulls":6},"     起重量300kN及以上的起重设备安装工程；高度200m及以上内爬起重\r\n 设备的拆除工程"]
[null,4," 脚手架工程",null,null,null,"     搭设高度50m及以上的落地式钢管脚手架工程"]
[{"$nulls":6},"     提升高度150m及以上附着式整体和分片提升脚手架工程"]
[{"$nulls":6},"     架体高度20m及以上悬挑式脚手架工程"]
[null,5," 拆除、爆破工程",null,null,null,"     采用爆破拆除的工程"]
[{"$nulls":6},"     码头、桥梁、高架、烟囱、水塔或拆除中容易引起有毒有害气(液)体\r\n 或粉尘扩散、易燃易爆事故发生的特殊建、构筑物的拆除工程"]
[{"$nulls":6},"     可能影响行人、交通、电力设施、通信设施或其他建、构筑物安全的\r\n 拆除工程"]
[{"$nulls":6},"     文物保护建筑、优秀历史建筑或历史文化风貌区控制范围的拆除工程"]
[null,6," 其他危险性较大\r\n 的工程",null,null,null,"     施工高度50m及以上的建筑幕墙安装工程"]
[{"$nulls":6},"     跨度大于36m及以上的钢结构安装工程；跨度大于60m及以上的网架和\r\n 索膜结构安装工程"]
[{"$nulls":6},"     开挖深度超过16m的人工挖扩孔桩工程"]
[{"$nulls":6},"     地下暗挖工程、顶管工程、水下作业工程"]
[{"$nulls":6},"     采用新技术、新工艺、新材料、新设备及尚无相关技术标准的危险性\r\n 较大的分部分项工程"]
[null," 施工总包单位(公章):",{"$nulls":10},"监理单位项目部(盖章):"]
[null," 项目负责人（签名）:",{"$nulls":10},"总监理工程师（签名）："]
[{"$nulls":19},"年  月  日"]
[null," 注:含有的打“√”，没有的打“×”，由总包单位填写，监理单位确认。"]